**K32     PANEL CUBICLES**

**120      PANEL CUBICLES - UNFRAMED**

**Manufacturer:** Formwise Washrooms Ltd, Unit 3 Wendel Point, Park Farm, Wellingborough, Northamptonshire NN8 6BA

T: 01933 405961 F: 01933 405971

Email: sales@formwise-washrooms.co.uk

Web: [www.formwise-washrooms.co.uk](http://www.formwise-washrooms.co.uk)

**Product reference:** ‘**butterfly sgl’ children’s** toilet cubicles

**Panels/ Doors & Pilasters:** 12/13mm solid grade laminate (SGL) to provide maximum protection against water and vandalism.

**Core material:** Not applicable.

**Finish:** Velour.

**Colour:** Colour to be confirmed from Formwise Washrooms SGL selection.

**Edge treatment:** Edges are machined to a smooth profiled finish.

**Headrails:** Rigid polished aluminium section with bull-nosed leading edge.

**Legs:** Tubular polished aluminium design, through fixed into front of pilaster. Adjustable to accommodate varying floor levels.

**Ironmongery/ Accessories:** Aluminium pivot hinges with increased finger protection / Coat hook / DDA compliant slide operated indicator bolt with elliptical face plate / Emergency release facility. Channel bracket partition fixings.

**Finish/ Colour:** Polished.

**Dimensions:** 1980mm overall height including 160mm floor clearance.

**Other requirements:** Doors & Pilasters to be shaped to form a curve, and partitions machined to sweep up towards the full size pilasters.

Complete with outward opening doors to ambulant and enlarged cubicles where requested. Cubicles with inward opening doors can be set out to maintain 450mm diameter manoeuvring space within the cubicle.