**K32     PANEL CUBICLES**

**120      PANEL CUBICLES – UNFRAMED**

**Manufacturer:** Formwise Washrooms Ltd, Unit 3 Wendel Point, Park Farm, Wellingborough, Northamptonshire

NN8 6QJ. T: 01933 405961 F: 01933 405971

Email: sales@formwise-washrooms.co.uk

Web: [www.formwise-washrooms.co.uk](http://www.formwise-washrooms.co.uk)

**Product reference:** ‘**form hpl’** toilet cubicles

**Doors:** 30mm chipboard faced both sides with high pressure laminate (HPL).

**Core material:** High density chipboard.

**Finish:** Velour.

**Colour:** Colour to be confirmed from Formwise Washrooms HPL selection.

**Edge treatment:** All edges are lipped square.

**Panels:** 30mm chipboard faced both sides with high pressure laminate (HPL).

**Core material:** High density chipboard.

**Finish:** Velour.

**Colour:** Colour to be confirmed from Formwise Washrooms HPL selection.

**Edge treatment:** Leading edge of extended partition is bullnosed to 180 degree profile, all other edges are lipped square.

**Pilasters:** Two formed stainless steel angle profiles fixed to either side of the partition and set back from leading edge. Vertical edges are full radiused for safety.

**Finish:** Satin polished.

**Colour:** Self coloured.

            **Headrails:** 25mm diameter stainless steel tube fixed between partitions.

**Legs:** Slimline, cylindrical design, with concealed fixings. Adjustable to accommodate varying floor levels.

**Ironmongery/ Accessories:** Adjustable pivot hinges / Buffered coat hook / DDA compliant lever operated indicator bolt with circular face plate and emergency release facility / Concealed continuous ‘T’ section partition fixings.

**Finish/ Colour:** Stainless steel or stainless steel effect.

**Dimensions:** 2100mm overall height including 100mm floor clearance.

**Other requirements:** Complete with outward opening doors to ambulant and enlarged cubicles where requested. Cubicles with inward opening doors can be set out to maintain 450mm diameter manoeuvring space within the cubicle, this may require an extended pilaster detail.