**K32     PANEL CUBICLES**

**120      PANEL CUBICLES – UNFRAMED**

**Manufacturer:** Formwise Washrooms Ltd, Unit 3 Wendel Point, Park Farm, Wellingborough, Northamptonshire

NN8 6QJ. T: 01933 405961 F: 01933 405971

Email: sales@formwise-washrooms.co.uk

Web: [www.formwise-washrooms.co.uk](http://www.formwise-washrooms.co.uk)

**Product reference:** ‘**form sgl’** toilet cubicles

**Panels & Doors:** 12/13mm solid grade laminate (SGL) to provide maximum protection against water and vandalism.

**Core material:** Not applicable.

**Finish:** Velour.

**Colour:** Colour to be confirmed from Formwise Washrooms SGL selection.

**Edge treatment:** Edges are machined to a smooth profiled finish.

**Pilasters:** Two formed stainless steel angle profiles fixed to either side of the partition and set back from leading edge. Vertical edges are full radiused for safety.

**Finish:** Satin polished.

**Colour:** Self coloured.

            **Headrails:** 25mm diameter stainless steel tube fixed between partitions.

**Legs:** Slimline, cylindrical design. Adjustable to accommodate varying floor levels.

**Ironmongery/ Accessories:** Adjustable pivot hinges / Buffered coat hook / DDA compliant lever operated indicator bolt with circular face plate and emergency release facility / Channel bracket partition fixings.

**Finish/ Colour:** Stainless steel or stainless steel effect.

**Dimensions:** 2100mm overall height including 100mm floor clearance.

**Other requirements:** Complete with outward opening doors to ambulant and enlarged cubicles where requested. Cubicles with inward opening doors can be set out to maintain 450mm diameter manoeuvring space within the cubicle, this may require an extended pilaster detail.