**K32     PANEL CUBICLES**

**120      PANEL CUBICLES - UNFRAMED**

**Manufacturer:** Formwise Washrooms Ltd, Unit 3 Wendel Point, Park Farm, Wellingborough, Northamptonshire NN8 6BA

T: 01933 405961 F: 01933 405971 Email: [sales@formwise-washrooms.co.uk](mailto:sales@formwise-washrooms.co.uk)

Web: [www.formwise-washrooms.co.uk](http://www.formwise-washrooms.co.uk)

**Product reference:** ‘**function hpl’** toilet cubicles

**Panels/ Doors & Pilasters:** 18mm moisture resistant chipboard faced both sides with high pressure laminate (HPL).

**Core material:** Moisture resistant chipboard (to V313).

**Finish:** Velour.

**Colour:** Colour to be confirmed from Formwise Washrooms HPL selection.

**Edge treatment:** All edges are lipped with matching / contrasting

durable PVC.

**Headrail:** Rigid polished aluminium section with bull-nosed leading edge.

**Legs:** Polished aluminium rectangular design, partition fixed. Adjustable to accommodate varying floor levels.

**Ironmongery/ Accessories:** Aluminium pivot hinges / Coat hook / DDA compliant slide operated indicator bolt with elliptical face plate / Emergency release facility. Channel bracket partition fixings.

**Finish/ Colour:** Polished.

**Dimensions:** 1980mm overall height including 160mm floor clearance.

**Other requirements:** Complete with outward opening doors to ambulant and enlarged cubicles where requested. Cubicles with inward opening doors can be set out to maintain 450mm diameter manoeuvring space within the cubicle.