**K32     PANEL CUBICLES**

**120      PANEL CUBICLES - UNFRAMED**

**Manufacturer:** Formwise Washrooms Ltd, Unit 3 Wendel Point, Ryle drive, Park Farm, Wellingborough, Northamptonshire NN8 6BA.

T: 01933 405961 F: 01933 405971

Email: sales@formwise-washrooms.co.uk

Web: [www.formwise-washrooms.co.uk](http://www.formwise-washrooms.co.uk)

**Product reference:** ‘**hoxton’** toilet cubicles

**Partitions:** 12/13mm solid grade laminate (SGL) to provide maximum protection against water and vandalism

**Core material:** Not applicable.

**Finish:** Velour.

**Colour:** Colour to be confirmed from Formwise Washrooms SGL selection.

**Edge treatment:** Edges are a machined finish.

**Doors & Pilasters:** 12/13mm solid grade laminate (SGL) to provide maximum protection against water and vandalism

**Core material:** Not applicable.

**Finish:** Velour.

**Colour:** Colour to be confirmed from Formwise Washrooms SGL selection.

**Edge treatment:** Vertical edges are rebated to enable the doors to close flush with the adjacent pilasters.

**Headrail:** Stainless steel rectangular section.

**Legs:** Cylindrical brushed stainless steel pedestal leg set on cubicle division

**Ironmongery/ Accessories:** Sprung action stainless steel hinges / Buffered coat hook / DDA compliant lever operated indicator bolt with circular face plate and emergency release facility / Channel bracket partition fixings

**Finish/ Colour:** Brushed stainless steel

**Dimensions:** 2000mm overall height including 160mm floor clearance.

**Other requirements:** Complete with outward opening doors to ambulant and enlarged cubicles where requested. Cubicles with inward opening doors can be set out to maintain 450mm diameter manoeuvring space within the cubicle.