**N10 GENERAL FIXTURES/ FURNISHINGS/ EQUIPMENT**

**145A VANITY UNITS**

**Manufacturer:** Formwise Washrooms Ltd, Unit 3 Wendel Point, Park Farm, Wellingborough, Northamptonshire NN8 6BA

T: 01933 405961 F: 01933 405971

Email: [sales@formwise-washrooms.co.uk](mailto:sales@formwise-washrooms.co.uk)

Web: [www.formise-washrooms.co.uk](http://www.formise-washrooms.co.uk)

**Product reference: ‘HPL Vanity V1’** vanity unit system

**Dimensions:** 800mm high x max 3600mm un-jointed lengths subject to site access.

**Vanity top material**: 600mm bed manufactured from high pressure laminate bonded to 18mm Moisture resistant chipboard with backing laminate.

**Finish / Colour**: Colour from Formwise Washrooms HPL range of laminates, finish velour.

**Front edge profile**: Front edge postformed with 200mm downstand.

**Rear edge profile**: Postformed to form coved upstand up to 100mm high.

**Underpanel material:** 18mm moisture resistant V313 chipboard faced both sides with high pressure laminate.

**Finish/colour:** Colour to be confirmed from Formwise Washrooms HPL selection.

**Edge treatment:** All edges are lipped with matching/contrasting durable 1mm PVC.

**Accessories:** Concealed Keku ‘lift off’ brackets.

**Support system:** Treated softwood framework, notched and screwed made to measure and site assembled.

**Other requirements:** Not applicable.