**K13     PANEL CUBICLES**

**160      PROPRIETARY PANEL LINING SYSTEMS**

**Substrate:** Treated softwood framework, notched and screwed made to measure and site assembled.

**Panels:**

**Manufacturer:** Formwise Washrooms Ltd, Unit 3 Wendel Point, Park Farm, Wellingborough, Northamptonshire NN8 6BA

T: 01933 405961 F: 01933 405971

Email: [sales@formwise-washrooms.co.uk](mailto:sales@formwise-washrooms.co.uk)

Web: [www.formwise-washrooms.co.uk](http://www.formwise-washrooms.co.uk)

**Product reference:** ‘**mfc’** duct / access panelling.

**Board /Panels:** Melamine faced made to measure panels, full height three panel sets.

**Thickness:** 19mm.

**Core material:** Moisture resistant (MR) melamine faced 710kg/m3 chipboard (MFC).

**Facing:** Melamine.

**Colour:** Colour to be confirmed from Formwise Washrooms MFC selection.

**Moisture content at time of fixing:** As recommended by fabricator to suit environmental conditions as clause. Consult with Formwise Washrooms for details.

**Edge treatment:** All edges lipped with matching/contrasting durable 1mm PVC.

**Installation:**

**Method of fixing panels :** Concealed Keku 'lift off' brackets.

**Joint treatment:** Supplied with horizontal and vertical flash gaps in black laminate.

**Included features:** All duct paneling / cistern duct sets to be made to suit site dimensions with vertical flashgaps kept to a minimum.

**Accessories:** All fixing components.