**K13     PANEL CUBICLES**

**160      PROPRIETARY PANEL LINING SYSTEMS**

**Substrate:** Treated softwood framework, notched and screwed made to measure and site assembled.

**Panels:**

**Manufacturer:** Formwise Washrooms Ltd, Unit 3 Wendel Point, Park Farm, Wellingborough, Northamptonshire NN8 6BA

T: 01933 405961 F: 01933 405971

Email: sales@formwise-washrooms.co.uk

Web: [www.formwise-washrooms.co.uk](http://www.formise-washrooms.co.uk)

**Product reference:** ‘**sgl’** duct / access panelling.

**Board /Panels:** Solid grade laminate made to measure panels, low level with two face panels and one shelf panel.

**Thickness:** 12/13mm overall

**Core material:** Not applicable

**Facing:** Not applicable

**Colour:** Colour to be confirmed from Formwise Washrooms SGL selection.

**Moisture content at time of fixing:** As recommended by fabricator to suit environmental conditions as clause consult with Amwell Systems for details

**Edge treatment:** Exposed edges are machined to a smooth profiled finish.

**Installation:**

**Method of fixing panels:** Concealed Keku ‘lift off’ brackets.

**Joint treatment:** With horizontal and vertical flash gaps (flashgap laminate can either match or contrast panel colour).

**Included features:** All duct paneling / cistern duct sets to be made to suit site dimensions with vertical flashgaps kept to a minimum

**Accessories:** All fixing components.