**K32     PANEL CUBICLES**

**120     PANEL CUBICLES - UNFRAMED**

**Manufacturer:** Formwise Washrooms Ltd, Unit 3 Wendel Point, Park Farm, Wellingborough, Northamptonshire NN8 6BA

T: 01933 405961 F: 01933 405971

Email: sales@formwise-washrooms.co.uk

Web: [www.formwise-washrooms.co.uk](http://www.formwise-washrooms.co.uk)

**Product reference:** **‘caterpillar sgl’ children’s** toilet cubicles.

**Panels/ Doors:** 12/13mm Solid grade laminate (SGL) to provide maximum protection against water and vandalism.

**Core material:** Not Applicable.

**Finish:** Velour.

**Colour:** Colour to be confirmed from Formwise Washrooms SGL selection.

**Edge treatment:** Edges are machined to a smooth profiled finish.

**Ironmongery/ Accessories:** Aluminium pivot hinges with increased finger protection / Powder coated pilaster floor fixing / Internal handle and magnetic catches / Coat hook / Channel bracket partition fixings.

**Finish/ Colour:** Polished.

**Dimensions: Option A:**1100mm overall height including 100mm floor clearance.

**Option B:**1350mm overall height including 100mm floor clearance.

**Other requirements:** Doors and pilasters to be shaped to form a curve, and partitions machined to sweep up towards the pilasters. Complete with outward opening doors to ambulant and enlarged cubicles where requested. Cubicles with inward opening doors can be set out to maintain 450mm diameter manoeuvring space within the cubicle.