**N10 GENERAL FIXTURES/ FURNISHINGS/ EQUIPMENT**

**145A VANITY UNITS**

**Manufacturer:** Formwise Washrooms Ltd, Unit 3 Wendel Point, Park Farm, Wellingborough, Northamptonshire NN8 6BA

T: 01933 405961 F: 01933 405971

Email: [sales@formwise-washrooms.co.uk](mailto:sales@formwise-washrooms.co.uk)

Web: [www.formwise-washrooms.co.uk](http://www.formwise-washrooms.co.uk)

**Product reference: ‘SGL’** vanity unit system

**Dimensions:** 800mm high x max 3600mm un-jointed lengths subject to site access.

**Vanity tops material:** 600mm wide bed manufactured from solid grade laminate (SGL).

**Finish/ colour:** Colour to be confirmed from Formwise Washrooms SGL selection, finish velour.

**Front edge profile:** Aluminium section profiled finish with a 200mm downstand.

**Rear edge profile:** 100mm high rear upstand with a coved aluminium profile section

**Underpanel material:** 12/13mm solid grade laminate (SGL) to provide maximum protection against water and vandalism.

**Finish/colour:** Colour to be confirmed from Formwise Washrooms SGL selection, finish velour.

**Edge treatment:** Edges are machined to a smooth profiled finish.

**Accessories:** Concealed Keku ‘lift off’ brackets.

**Support system:** Treated softwood framework, notched and screwed made to measure and site assembled.

**Other requirements:** Not applicable